


Public Involvement - Narrative Template (Canoe Creek) 

1. Cover (Slide 1)
This is the Public Involvement presentation for the Alabama Department of Transportation Project BR-I059(445) Bridge replacement on Interstate 59 over Canoe Creek in St. Clair County.

2. Welcome (Slide 2)
Welcome and thank you for participating in the online public involvement for the proposed improvements on Interstate 59 in St. Clair County, Alabama.  We want to provide an opportunity for you to review and comment on the proposed project. Your input is crucial to the advancement of this project. The information provided within this presentation is preliminary and subject to change. 

3. Project Location (Slide 3)
The Alabama Department of Transportation is proposing to replace the bridges on Interstate 59 over Canoe Creek in St. Clair County. The proposed project is located along the interstate between the cities of Springville and Ashville.  The interstate is a divided roadway with two travel lanes in each direction within the project corridor.  The terrain in the project corridor is wooded and undeveloped.

4. Purpose and Need (Slide 4)
The existing bridges were constructed in the early 1960’s.  The bridges have two - 12 ft travel lanes and 4 ft shoulders.  The current structures are damaged and too narrow to accommodate current vehicles.  The new structures are proposed to address the deteriorating condition of the bridges and to preserve a safer and more efficient transportation system.

5. Project Description Scope of Work (Slide 5) 

The new bridges will be built on the existing alignment.  The new bridges will be approximately 485 ft long and 54 ft wide to accommodate 2 – 12 ft lanes and 2 – 15 ft shoulders.  

The approach roadway to the bridges will be accessible and remain in use during construction. 
Staged construction is proposed for this project; one lane of the bridges in each direction will remain open and be accessible during the project.




	
6. Project Schedule (Impacts) (Slide 6) 

The acquisition of additional right-of-way, temporary construction easements and utility relocations will not be required to replace these bridges. 

Construction of the new bridge and approaches will tentatively begin Winter of 2027. 

Staged construction is proposed.  One lane across the bridge in each direction will be accessible during construction. 

No detours are planned or anticipated for this project.

 Construction is anticipated to take approximately 18-24 months.

7. Public Involvement (Slide 7)
There will not be an in-person public involvement meeting.  You can make inquiries and/or    	 provide your comments regarding this project online, by voice mail, fax or US mail as    	                       noted.  Please provide your comments by Friday, September 18, 2026.

8.  Thank you (Slide 8)
If you should have any questions or require additional information, please contact our 	  
 Communications and Public Relations Coordinator, Jon Paepcke.
         We appreciate your interest and participation.  Thank you.



